FILE_TYPE = MULTI_PHYS_TABLE;

PART 'MAX485ESA_T'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "ARROW_PART_NUMBER", "ARROW_PRICE/STOCK", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Maxim Integrated", "MAX485ESA+T" (!) = "", "SOIC127P600X175-8N", "Small Outline Packages", "", "", "700-MAX485ESAT", "https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX485ESA%2bT?qs=LHmEVA8xxfYXmvxEk%252BFtEg%3D%3D", "RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers", "https://datasheets.maximintegrated.com/en/ds/MAX1487-MAX491.pdf", "1.75 mm"
END_PART

END.
