(part "C0805C104K5RAC7411"
    (packageRef "CAPC2012X88N")
    (interface
        (port "1" (symbPinId 1) (portName "1") (portType INOUT))
        (port "2" (symbPinId 2) (portName "2") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "compKind" "32")
    (property "Manufacturer_Name" "Kemet")
    (property "Manufacturer_Part_Number" "C0805C104K5RAC7411")
    (property "Arrow_Part_Number" "C0805C104K5RAC7411")
    (property "Arrow_Price/Stock" "https://www.arrow.com/en/products/c0805c104k5rac7411/kemet-corporation")
    (property "Mouser_Part_Number" "80-C0805C104K5RACLR")
    (property "Mouser_Price/Stock" "https://www.mouser.co.uk/ProductDetail/KEMET/C0805C104K5RAC7411?qs=jbRM9o5BbzPcVXF0wW9AYg%3D%3D")
    (property "Description" "Cap Ceramic 0.1uF 50V X7R 10% Pad SMD 0805 125C T/R")
    (property "Datasheet_Link" "https://www.mouser.com/datasheet/2/212/KEM_C1002_X7R_SMD-1102033.pdf")
    (property "symbolName1" "C0805C104K5RAC7411")
)
