FILE_TYPE = MULTI_PHYS_TABLE;

PART 'C0805X106K8RACAUTO'
CLASS = DISCRETE
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "ARROW_PART_NUMBER", "ARROW_PRICE/STOCK", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Kemet", "C0805X106K8RACAUTO" (!) = "", "CAPC2012X100N", "Capacitor Chip Non-polarised", "C0805X106K8RACAUTO", "https://www.arrow.com/en/products/c0805x106k8racauto/kemet-corporation", "80-C0805X106K8RAUTO", "https://www.mouser.co.uk/ProductDetail/KEMET/C0805X106K8RACAUTO?qs=HXFqYaX1Q2z3R2ozxnMwnQ%3D%3D", "Multilayer Ceramic Capacitors MLCC - SMD/SMT 10V 10uF X7R 0805 10% AEC-Q200", "https://mouser.componentsearchengine.com/Datasheets/1/C0805X106K8RACAUTO.pdf", "1 mm"
END_PART

END.
