<?xml version="1.0" encoding="utf-8"?>
<!--/231688/311096/2.47/8/4/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOIC127P600X175-8N">
<description>&lt;b&gt; 8 SO&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="MAX485ESA+T">
<pin name="RO" direction="io"/>
<pin name="!RE" direction="io"/>
<pin name="DE" direction="io"/>
<pin name="DI" direction="io"/>
<pin name="VCC" direction="io"/>
<pin name="B" direction="io"/>
<pin name="A" direction="io"/>
<pin name="GND" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX485ESA+T" prefix="IC">
<description>&lt;b&gt;RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://datasheets.maximintegrated.com/en/ds/MAX1487-MAX491.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="MAX485ESA+T"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="Manufacturer_Name" value="Maxim Integrated"/>
<attribute name="Manufacturer_Part_Number" value="MAX485ESA+T"/>
<attribute name="Arrow_Part_Number" value=""/>
<attribute name="Arrow_Price-Stock" value=""/>
<attribute name="Mouser_Part_Number" value="700-MAX485ESAT"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX485ESA%2bT?qs=LHmEVA8xxfYXmvxEk%252BFtEg%3D%3D"/>
<attribute name="Description" value="RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers"/>
<attribute name="Height" value="1.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
