
(EDIF
  (rename &CRCW08054K70FKEAC "CRCW08054K70FKEAC")
  (EDIFVersion 2 0 0)
  (EDIFLevel 0)
  (keywordMap (keywordLevel 0))
  (status
    (written
      (timestamp 2020 09 09 10 28 02)
      (dataOrigin "995989/311096/2.47/2/3/Resistor")
      (program "SamacSys ECAD Model CRCW08054K70FKEAC"
        (version "1.1"))))
  (library
  (rename &CRCW08054K70FKEAC "CRCW08054K70FKEAC")
    (EDIFLevel 0)
    (technology
      (numberDefinition (scale 1 (e 254 -6) (unit DISTANCE)))
      (userData GRIDRESOLUTION (integer 50 50))
      (figureGroup DEFAULT (pathWidth 10) (textHeight 100))
      (figureGroup PROPERTY (pathWidth 10) (textHeight 90))
      (figureGroup PINNUMBER (pathWidth 10) (textHeight 90))
      (figureGroup PINNAME (pathWidth 10) (textHeight 90))
      (figureGroup COMMENT (pathWidth 10) (textHeight 90))
      (figureGroup PIN (pathWidth 10) (textHeight 90))
      (figureGroup GRAPHIC (pathWidth 10) (textHeight 100))
    )
    (cell
      (rename &CRCW08054K70FKEAC "CRCW08054K70FKEAC")
      (cellType GENERIC)
      (view
        (rename NORMAL "Normal")
        (viewType SCHEMATIC)
        (interface
          (designator "R")
          (property (rename PACKAGENAME "PackageName") (string "CRCW08054K70FKEAC"))
          (property (rename ISHETEROGENEOUS "IsHeterogeneous") (string "False"))
          (property (rename DEVICESINVIEW "DevicesInView") (string "1"))
          (property (rename DEVICESINPACKAGE "DevicesInPackage") (string "1"))
          (property (rename DEVICEDESIGNATOR "DeviceDesignator") (string "A"))
          (property (rename DEVICENUMBERING "DeviceNumbering") (string "Alpha"))
          (property (rename PCB_32_FOOTPRINT "PCB Footprint") (string "RESC2012X60N"))
          (property (rename &Manufacturer_Name "Manufacturer_Name") (string "Vishay"))
          (property (rename &Manufacturer_Part_Number "Manufacturer_Part_Number") (string "CRCW08054K70FKEAC"))
          (property (rename &Arrow_Part_Number "Arrow Part Number") (string "CRCW08054K70FKEAC"))
          (property (rename &Arrow_Price_Stock "Arrow Price/Stock") (string "https://www.arrow.com/en/products/crcw08054k70fkeac/vishay"))
          (property (rename &Mouser_Part_Number "Mouser Part Number") (string "71-CRCW08054K70FKEAC"))
          (property (rename &Mouser_Price_Stock "Mouser Price/Stock") (string "https://www.mouser.co.uk/ProductDetail/Vishay-Dale/CRCW08054K70FKEAC?qs=E3Y5ESvWgWOQAAVugewEHA%3D%3D"))
          (property (rename &Description "Description") (string "Thick Film Resistors - SMD 1/8Watt 4.7Kohms 1percent Commercial Use"))
          (property (rename &Datasheet_Link "Datasheet Link") (string "https://mouser.componentsearchengine.com/Datasheets/1/CRCW08054K70FKEAC.pdf"))
          (property (rename &Height "Height") (string "0.6 mm"))
          (property (rename &_60__32_VALUE_32__62_ "Value") (string "CRCW08054K70FKEAC"))
          (property (rename VALUE "Value") (string "Value"))
          (port
            (rename &1 "1")
            (designator "1")
            (property (rename ORDER "Order") (string "0") (owner "OrCAD"))
          )
          (port
            (rename &2 "2")
            (designator "2")
            (property (rename ORDER "Order") (string "1") (owner "OrCAD"))
          )
          (symbol
            (portImplementation
              (name &1)
              (keywordDisplay DESIGNATOR (display PINNUMBER))
              (figure PIN (path (pointList (pt -200 -100) (pt 0 -100))))
              (connectLocation (figure GRAPHIC (dot (pt -200 -100))))
            )
            (portImplementation
              (name &2)
              (keywordDisplay DESIGNATOR (display PINNUMBER))
              (figure PIN (path (pointList (pt 300 -100) (pt 500 -100))))
              (connectLocation (figure GRAPHIC (dot (pt 500 -100))))
            )
            (figure GRAPHIC
              (figureGroupOverride GRAPHIC
                (pathWidth 10))
              (path
                (pointList
                  (pt 0 -50)
                  (pt 300 -50)
                  (pt 300 -150)
                  (pt 0 -150)
                  (pt 0 -50)
                )
              )
            )
            (keywordDisplay DESIGNATOR (display PROPERTY (justify LOWERLEFT) (orientation R0) (origin (pt 350 80))))
            (propertyDisplay &_60__32_VALUE_32__62_ (display PROPERTY (justify LOWERLEFT) (orientation R0) (origin (pt 350 -20))))
          )
        )
      )
    )
  )
)
