(export (version D)
  (design
    (source /Users/mn/Documents/test/test.sch)
    (date "2020 May 11, Monday 16:27:15")
    (tool "Eeschema (5.1.5-0-10_14)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source test.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J7)
      (value "DMX0 DI DE RE RO")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA115E))
    (comp (ref J11)
      (value "DMX0 VCC B A GND")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA477C))
    (comp (ref J8)
      (value "DMX1 DI DE RE RO")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA62A6))
    (comp (ref J12)
      (value "DMX1 VCC B A GND")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA6DA2))
    (comp (ref J9)
      (value "DMX2 DI DE RE RO")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA7AB2))
    (comp (ref J13)
      (value "DMX2 VCC B A GND")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA85AD))
    (comp (ref J10)
      (value "DMX3 DI DE RE RO")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA903B))
    (comp (ref J14)
      (value "DMX3 VCC B A GND")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBA980F))
    (comp (ref J17)
      (value "CMOD A7 J1")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x24_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x24) (description "Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBEF8A2))
    (comp (ref J18)
      (value "CMOD A7 J2")
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x24_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x24) (description "Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBF1AD7))
    (comp (ref J1)
      (value "FPGA PIN 1-12")
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_1-282834-2_1x12_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x12) (description "Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBF7475))
    (comp (ref J2)
      (value "FPGA PIN 13-24")
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_1-282834-2_1x12_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x12) (description "Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBFA515))
    (comp (ref J4)
      (value "FPGA PIN 37-48")
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_1-282834-2_1x12_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x12) (description "Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBFAF44))
    (comp (ref J5)
      (value "FPGA PIN 25-36")
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_1-282834-2_1x12_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x12) (description "Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBFCB16))
    (comp (ref J3)
      (value "Power Supply")
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x02) (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EBFFD2E))
    (comp (ref J6)
      (value LAN8720)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x07_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x07_Odd_Even) (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EDAE843)))
  (libparts
    (libpart (lib Connector) (part Screw_Terminal_01x02)
      (description "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Screw_Terminal_01x12)
      (description "Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x12))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x24)
      (description "Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x24))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x07_Odd_Even)
      (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x07_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri "/Library/Application Support/kicad/library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "/Library/Application Support/kicad/library/Connector_Generic.lib")))
  (nets
    (net (code 1) (name "Net-(J7-Pad1)")
      (node (ref J7) (pin 1)))
    (net (code 2) (name "Net-(J11-Pad2)")
      (node (ref J11) (pin 2)))
    (net (code 3) (name "Net-(J11-Pad3)")
      (node (ref J11) (pin 3)))
    (net (code 4) (name "Net-(J8-Pad1)")
      (node (ref J8) (pin 1)))
    (net (code 5) (name "Net-(J12-Pad2)")
      (node (ref J12) (pin 2)))
    (net (code 6) (name "Net-(J12-Pad3)")
      (node (ref J12) (pin 3)))
    (net (code 7) (name "Net-(J9-Pad1)")
      (node (ref J9) (pin 1)))
    (net (code 8) (name "Net-(J13-Pad2)")
      (node (ref J13) (pin 2)))
    (net (code 9) (name "Net-(J13-Pad3)")
      (node (ref J13) (pin 3)))
    (net (code 10) (name "Net-(J10-Pad1)")
      (node (ref J10) (pin 1)))
    (net (code 11) (name "Net-(J14-Pad2)")
      (node (ref J14) (pin 2)))
    (net (code 12) (name "Net-(J14-Pad3)")
      (node (ref J14) (pin 3)))
    (net (code 13) (name "Net-(J1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref J17) (pin 1)))
    (net (code 14) (name "Net-(J1-Pad10)")
      (node (ref J17) (pin 10))
      (node (ref J1) (pin 10)))
    (net (code 15) (name "Net-(J17-Pad15)")
      (node (ref J2) (pin 3))
      (node (ref J17) (pin 15)))
    (net (code 16) (name "Net-(J17-Pad16)")
      (node (ref J2) (pin 4))
      (node (ref J17) (pin 16)))
    (net (code 17) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2))
      (node (ref J17) (pin 2)))
    (net (code 18) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4))
      (node (ref J17) (pin 4)))
    (net (code 19) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5))
      (node (ref J17) (pin 5)))
    (net (code 20) (name "Net-(J1-Pad6)")
      (node (ref J17) (pin 6))
      (node (ref J1) (pin 6)))
    (net (code 21) (name "Net-(J1-Pad7)")
      (node (ref J17) (pin 7))
      (node (ref J1) (pin 7)))
    (net (code 22) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8))
      (node (ref J17) (pin 8)))
    (net (code 23) (name "Net-(J1-Pad9)")
      (node (ref J17) (pin 9))
      (node (ref J1) (pin 9)))
    (net (code 24) (name "Net-(J18-Pad1)")
      (node (ref J18) (pin 1))
      (node (ref J4) (pin 1)))
    (net (code 25) (name "Net-(J18-Pad10)")
      (node (ref J18) (pin 10))
      (node (ref J4) (pin 10)))
    (net (code 26) (name "Net-(J18-Pad11)")
      (node (ref J18) (pin 11))
      (node (ref J4) (pin 11)))
    (net (code 27) (name "Net-(J10-Pad4)")
      (node (ref J18) (pin 12))
      (node (ref J10) (pin 4))
      (node (ref J4) (pin 12)))
    (net (code 28) (name "Net-(J18-Pad13)")
      (node (ref J9) (pin 4))
      (node (ref J18) (pin 13))
      (node (ref J5) (pin 1)))
    (net (code 29) (name "Net-(J18-Pad14)")
      (node (ref J5) (pin 2))
      (node (ref J8) (pin 4))
      (node (ref J18) (pin 14)))
    (net (code 30) (name "Net-(J18-Pad15)")
      (node (ref J7) (pin 4))
      (node (ref J5) (pin 3))
      (node (ref J18) (pin 15)))
    (net (code 31) (name "Net-(J18-Pad16)")
      (node (ref J5) (pin 4))
      (node (ref J18) (pin 16)))
    (net (code 32) (name "Net-(J18-Pad17)")
      (node (ref J18) (pin 17))
      (node (ref J5) (pin 5)))
    (net (code 33) (name "Net-(J18-Pad18)")
      (node (ref J18) (pin 18))
      (node (ref J5) (pin 6)))
    (net (code 34) (name "Net-(J18-Pad19)")
      (node (ref J18) (pin 19))
      (node (ref J5) (pin 7)))
    (net (code 35) (name "Net-(J18-Pad2)")
      (node (ref J18) (pin 2))
      (node (ref J4) (pin 2)))
    (net (code 36) (name "Net-(J18-Pad20)")
      (node (ref J5) (pin 8))
      (node (ref J18) (pin 20)))
    (net (code 37) (name "Net-(J18-Pad21)")
      (node (ref J5) (pin 9))
      (node (ref J18) (pin 21)))
    (net (code 38) (name "Net-(J18-Pad22)")
      (node (ref J5) (pin 10))
      (node (ref J18) (pin 22)))
    (net (code 39) (name "Net-(J18-Pad23)")
      (node (ref J5) (pin 11))
      (node (ref J18) (pin 23)))
    (net (code 40) (name "Net-(J18-Pad3)")
      (node (ref J4) (pin 3))
      (node (ref J18) (pin 3)))
    (net (code 41) (name "Net-(J18-Pad4)")
      (node (ref J4) (pin 4))
      (node (ref J18) (pin 4)))
    (net (code 42) (name "Net-(J18-Pad5)")
      (node (ref J4) (pin 5))
      (node (ref J18) (pin 5)))
    (net (code 43) (name "Net-(J18-Pad6)")
      (node (ref J4) (pin 6))
      (node (ref J18) (pin 6)))
    (net (code 44) (name "Net-(J18-Pad7)")
      (node (ref J4) (pin 7))
      (node (ref J18) (pin 7)))
    (net (code 45) (name "Net-(J18-Pad8)")
      (node (ref J18) (pin 8))
      (node (ref J4) (pin 8)))
    (net (code 46) (name "Net-(J18-Pad9)")
      (node (ref J18) (pin 9))
      (node (ref J4) (pin 9)))
    (net (code 47) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3))
      (node (ref J17) (pin 3)))
    (net (code 48) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11))
      (node (ref J17) (pin 11)))
    (net (code 49) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12))
      (node (ref J17) (pin 12)))
    (net (code 50) (name "Net-(J17-Pad13)")
      (node (ref J2) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref J17) (pin 13)))
    (net (code 51) (name "Net-(J17-Pad17)")
      (node (ref J6) (pin 5))
      (node (ref J17) (pin 17))
      (node (ref J2) (pin 5)))
    (net (code 52) (name "Net-(J17-Pad18)")
      (node (ref J6) (pin 7))
      (node (ref J2) (pin 6))
      (node (ref J17) (pin 18)))
    (net (code 53) (name "Net-(J17-Pad19)")
      (node (ref J6) (pin 9))
      (node (ref J2) (pin 7))
      (node (ref J17) (pin 19)))
    (net (code 54) (name "Net-(J17-Pad22)")
      (node (ref J17) (pin 22))
      (node (ref J6) (pin 6))
      (node (ref J2) (pin 10)))
    (net (code 55) (name "Net-(J17-Pad23)")
      (node (ref J6) (pin 4))
      (node (ref J2) (pin 11))
      (node (ref J17) (pin 23)))
    (net (code 56) (name +5V)
      (node (ref J8) (pin 3))
      (node (ref J12) (pin 1))
      (node (ref J9) (pin 3))
      (node (ref J13) (pin 1))
      (node (ref J10) (pin 3))
      (node (ref J14) (pin 1))
      (node (ref J11) (pin 1))
      (node (ref J7) (pin 3))
      (node (ref J17) (pin 24))
      (node (ref J3) (pin 1))
      (node (ref J6) (pin 14))
      (node (ref J6) (pin 13))
      (node (ref J2) (pin 12)))
    (net (code 57) (name GND)
      (node (ref J8) (pin 2))
      (node (ref J6) (pin 11))
      (node (ref J6) (pin 12))
      (node (ref J5) (pin 12))
      (node (ref J12) (pin 4))
      (node (ref J9) (pin 2))
      (node (ref J3) (pin 2))
      (node (ref J18) (pin 24))
      (node (ref J7) (pin 2))
      (node (ref J13) (pin 4))
      (node (ref J11) (pin 4))
      (node (ref J10) (pin 2))
      (node (ref J14) (pin 4)))
    (net (code 58) (name "Net-(J6-Pad2)")
      (node (ref J6) (pin 2)))
    (net (code 59) (name "Net-(J17-Pad14)")
      (node (ref J6) (pin 3))
      (node (ref J2) (pin 2))
      (node (ref J17) (pin 14)))
    (net (code 60) (name "Net-(J17-Pad21)")
      (node (ref J17) (pin 21))
      (node (ref J6) (pin 8))
      (node (ref J2) (pin 9)))
    (net (code 61) (name "Net-(J17-Pad20)")
      (node (ref J17) (pin 20))
      (node (ref J6) (pin 10))
      (node (ref J2) (pin 8)))))