(part "C0805X106K8RACAUTO"
    (packageRef "CAPC2012X100N")
    (interface
        (port "1" (symbPinId 1) (portName "1") (portType INOUT))
        (port "2" (symbPinId 2) (portName "2") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "compKind" "32")
    (property "Manufacturer_Name" "Kemet")
    (property "Manufacturer_Part_Number" "C0805X106K8RACAUTO")
    (property "Arrow_Part_Number" "C0805X106K8RACAUTO")
    (property "Arrow_Price/Stock" "https://www.arrow.com/en/products/c0805x106k8racauto/kemet-corporation")
    (property "Mouser_Part_Number" "80-C0805X106K8RAUTO")
    (property "Mouser_Price/Stock" "https://www.mouser.co.uk/ProductDetail/KEMET/C0805X106K8RACAUTO?qs=HXFqYaX1Q2z3R2ozxnMwnQ%3D%3D")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 10V 10uF X7R 0805 10% AEC-Q200")
    (property "Datasheet_Link" "https://mouser.componentsearchengine.com/Datasheets/1/C0805X106K8RACAUTO.pdf")
    (property "symbolName1" "C0805X106K8RACAUTO")
)
