17330189010891
TerminalBlock_TE-Connectivity
TerminalBlock_TE_1-282834-0_1x10_P2.54mm_Horizontal
Terminal Block TE 1-282834-0, 10 pins, pitch 2.54mm, size 25.86x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 1-282834-0 pitch 2.54mm size 25.86x6.5mm^2 drill 1.1mm pad 2.1mm
0
10
10
TerminalBlock_TE-Connectivity
TerminalBlock_TE_1-282834-1_1x11_P2.54mm_Horizontal
Terminal Block TE 1-282834-1, 11 pins, pitch 2.54mm, size 28.4x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 1-282834-1 pitch 2.54mm size 28.4x6.5mm^2 drill 1.1mm pad 2.1mm
0
11
11
TerminalBlock_TE-Connectivity
TerminalBlock_TE_1-282834-2_1x12_P2.54mm_Horizontal
Terminal Block TE 1-282834-2, 12 pins, pitch 2.54mm, size 30.94x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 1-282834-2 pitch 2.54mm size 30.94x6.5mm^2 drill 1.1mm pad 2.1mm
0
12
12
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal
Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm
0
2
2
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-3_1x03_P2.54mm_Horizontal
Terminal Block TE 282834-3, 3 pins, pitch 2.54mm, size 8.08x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-3 pitch 2.54mm size 8.08x6.5mm^2 drill 1.1mm pad 2.1mm
0
3
3
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal
Terminal Block TE 282834-4, 4 pins, pitch 2.54mm, size 10.620000000000001x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-4 pitch 2.54mm size 10.620000000000001x6.5mm^2 drill 1.1mm pad 2.1mm
0
4
4
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-5_1x05_P2.54mm_Horizontal
Terminal Block TE 282834-5, 5 pins, pitch 2.54mm, size 13.16x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-5 pitch 2.54mm size 13.16x6.5mm^2 drill 1.1mm pad 2.1mm
0
5
5
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-6_1x06_P2.54mm_Horizontal
Terminal Block TE 282834-6, 6 pins, pitch 2.54mm, size 15.7x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-6 pitch 2.54mm size 15.7x6.5mm^2 drill 1.1mm pad 2.1mm
0
6
6
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-7_1x07_P2.54mm_Horizontal
Terminal Block TE 282834-7, 7 pins, pitch 2.54mm, size 18.240000000000002x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-7 pitch 2.54mm size 18.240000000000002x6.5mm^2 drill 1.1mm pad 2.1mm
0
7
7
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-8_1x08_P2.54mm_Horizontal
Terminal Block TE 282834-8, 8 pins, pitch 2.54mm, size 20.78x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-8 pitch 2.54mm size 20.78x6.5mm^2 drill 1.1mm pad 2.1mm
0
8
8
TerminalBlock_TE-Connectivity
TerminalBlock_TE_282834-9_1x09_P2.54mm_Horizontal
Terminal Block TE 282834-9, 9 pins, pitch 2.54mm, size 23.32x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity
THT Terminal Block TE 282834-9 pitch 2.54mm size 23.32x6.5mm^2 drill 1.1mm pad 2.1mm
0
9
9
