(export (version D)
  (design
    (source "F:\\Google Drive\\KiCad\\Artnet-LED\\LED Strip\\LED Strip.sch")
    (date "01.12.2020 16:07:01")
    (tool "Eeschema (5.1.5)-3")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "LED Strip.sch")
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref IC1)
      (value MAX485ESA+T)
      (footprint MAX485ESA+T:SOIC127P600X175-8N)
      (datasheet https://datasheets.maximintegrated.com/en/ds/MAX1487-MAX491.pdf)
      (fields
        (field (name Description) "RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers")
        (field (name Height) 1.75)
        (field (name Manufacturer_Name) "Maxim Integrated")
        (field (name Manufacturer_Part_Number) MAX485ESA+T)
        (field (name "Mouser Part Number") 700-MAX485ESAT)
        (field (name "Mouser Price/Stock") https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX485ESA%2bT?qs=LHmEVA8xxfYXmvxEk%252BFtEg%3D%3D))
      (libsource (lib LED-Strip-rescue) (part MAX485ESA+T-MAX485ESA+T) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 646DCA8A))
    (comp (ref C1)
      (value C100n)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib pspice) (part C) (description "Capacitor symbol for simulation only"))
      (sheetpath (names /) (tstamps /))
      (tstamp 646E2BDE))
    (comp (ref J2)
      (value Screw_Terminal_01x04)
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x04) (description "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 646E413C))
    (comp (ref J1)
      (value Screw_Terminal_01x04)
      (footprint TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Screw_Terminal_01x04) (description "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 646E5607))
    (comp (ref R4)
      (value R20k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F88C099))
    (comp (ref R3)
      (value R20k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F88D188))
    (comp (ref R5)
      (value R120)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F8908CE)))
  (libparts
    (libpart (lib Connector) (part Screw_Terminal_01x04)
      (description "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib LED-Strip-rescue) (part MAX485ESA+T-MAX485ESA+T)
      (fields
        (field (name Reference) IC)
        (field (name Value) MAX485ESA+T-MAX485ESA+T)
        (field (name Footprint) SOIC127P600X175-8N)
        (field (name Datasheet) https://datasheets.maximintegrated.com/en/ds/MAX1487-MAX491.pdf)
        (field (name Description) "RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers")
        (field (name Height) 1.75)
        (field (name Manufacturer_Name) "Maxim Integrated")
        (field (name Manufacturer_Part_Number) MAX485ESA+T)
        (field (name "Mouser Part Number") 700-MAX485ESAT)
        (field (name "Mouser Price/Stock") https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX485ESA%2bT?qs=LHmEVA8xxfYXmvxEk%252BFtEg%3D%3D))
      (pins
        (pin (num 1) (name RO) (type passive))
        (pin (num 2) (name ~RE) (type passive))
        (pin (num 3) (name DE) (type passive))
        (pin (num 4) (name DI) (type passive))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name A) (type passive))
        (pin (num 7) (name B) (type passive))
        (pin (num 8) (name VCC) (type passive))))
    (libpart (lib pspice) (part CAP)
      (aliases
        (alias C))
      (description "Capacitor symbol for simulation only")
      (docs ~)
      (fields
        (field (name Reference) C)
        (field (name Value) CAP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical LED-Strip-rescue)
      (uri "F:\\Google Drive\\KiCad\\Artnet-LED\\LED Strip/LED Strip-rescue.lib"))
    (library (logical pspice)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/pspice.lib")))
  (nets
    (net (code 1) (name "Net-(IC1-Pad1)")
      (node (ref IC1) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 3)))
    (net (code 2) (name GND)
      (node (ref IC1) (pin 5))
      (node (ref IC1) (pin 3))
      (node (ref IC1) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 4))
      (node (ref C1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 3) (name +5V)
      (node (ref C1) (pin 2))
      (node (ref IC1) (pin 4))
      (node (ref IC1) (pin 8))
      (node (ref J1) (pin 4))
      (node (ref R4) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 4) (name "Net-(IC1-Pad6)")
      (node (ref R5) (pin 2))
      (node (ref J2) (pin 3))
      (node (ref R4) (pin 2))
      (node (ref IC1) (pin 6)))
    (net (code 5) (name "Net-(IC1-Pad7)")
      (node (ref IC1) (pin 7))
      (node (ref R3) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref R5) (pin 1)))))