(part "MAX485ESA+T"
    (packageRef "SOIC127P600X175-8N")
    (interface
        (port "1" (symbPinId 1) (portName "RO") (portType INOUT))
        (port "2" (symbPinId 2) (portName "%RE%") (portType INOUT))
        (port "3" (symbPinId 3) (portName "DE") (portType INOUT))
        (port "4" (symbPinId 4) (portName "DI") (portType INOUT))
        (port "5" (symbPinId 5) (portName "GND") (portType INOUT))
        (port "6" (symbPinId 6) (portName "A") (portType INOUT))
        (port "7" (symbPinId 7) (portName "B") (portType INOUT))
        (port "8" (symbPinId 8) (portName "VCC") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "compKind" "101")
    (property "Manufacturer_Name" "Maxim Integrated")
    (property "Manufacturer_Part_Number" "MAX485ESA+T")
    (property "Arrow_Part_Number" "")
    (property "Arrow_Price/Stock" "")
    (property "Mouser_Part_Number" "700-MAX485ESAT")
    (property "Mouser_Price/Stock" "https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX485ESA%2bT?qs=LHmEVA8xxfYXmvxEk%252BFtEg%3D%3D")
    (property "Description" "RS-422/RS-485 Interface IC Low-Power, Slew-Rate-Limited RS-485/RS-422 Transceivers")
    (property "Datasheet_Link" "https://datasheets.maximintegrated.com/en/ds/MAX1487-MAX491.pdf")
    (property "symbolName1" "MAX485ESA+T")
)
